CFE version 1.0.37-0.7 for BCM96348 (32bit,SP,BE)                                                 
Build Date: Thu Mar  2 16:45:45 CST 2006 (root@hp)                                                  
Copyright (C) 2000,2001,2002,2003 Broadcom Corporation.                                                       

Initializing Arena.                   
Initializing Devices.                     
Flash device ID:235b                    
SST FLASH FAMILY                
Auto-negotiation timed-out                          
10 MB Half-Duplex (assumed)                           
CPU type 0x29107: 256MHz, Bus: 128MHz, Ref: 32MHz                                                 

Total memory used by CFE:  0x80401000 - 0x805232F0 (1188592)                                                            
Initialized Data:          0x8041B390 - 0x8041CC60 (6352)                                                         
BSS Area:                  0x8041CC60 - 0x804212F0 (180                                                      
Local Heap:                0x804212F0 - 0x805212F0 (1048576)                                                            
Stack Area:                0x805212F0 - 0x805232F0 (8192)                                                         
Text (code) segment:       0x80401000 - 0x8041B388 (107400)                                                           
Boot area (physical):      0x00524000 - 0x00564000                                                  
Relocation Factor:         I:00000000 - D:00000000                                                  

Board IP address                : 192.168.1.1:ffffff00                                                      
Host IP address                 : 192.168.1.100                                               
Gateway IP address              :                                 
Run from flash/host (f/h)       : f                                   
Default host run file name      : vmlinux                                         
Default host flash file name    : bcm963xx_fs_kernel                                                    
Boot delay (0-9 seconds)        : 1                                   
Board Id Name                   : 96348GW                                         
Psi size in KB                  : 24                                    
Number of MAC Addresses (1-32)  : 12                                    
Base MAC Address                : 00:16:38:fb:dd:2e                                                   
Ethernet PHY Type               : Internal                                          
Memory size in MB               : 16                                    

*** Press any key to stop auto run (1 seconds) ***                                                  
Auto run second count down: 0                             
Code Address: 0x80010000, Entry Address: 0x80188018                                                   
Decompression OK!                 
Entry at 0x80188018                   
Closing ne         
Starting program at 0x80188018                              
Linux version 2.6.8.1 (root@hp) (gcc version 3.4.2) #1 Wed Apr 5 20:10:01 CST 20                                                                                
06  
Flash device ID:235b                    
SST FLASH FAMILY                
Total Flash size: 4096K with 1024 sectors                                         
96348GW prom init                 
CPU revision is: 00029107                         
mpi: No Card is in the PCMCIA slot                                  
Determined physical RAM map:                            
 memory: 00fa0000 @ 00000000 (usable)                                     
On node 0 totalpages: 4000                          
  DMA zone: 4000 pages, LIFO batch:1                                    
  Normal zone: 0 pages, LIFO batch:1                                    
  HighMem zone: 0 pages, LIFO batch:1                                     
Built 1 zonelists                 
Kernel command line: r                     
brcm mips: enabling icache and dcache...                                        
Primary instruction cache 16kB, physically tagged, 2-way, linesize 16 bytes.                                                                            
Primary data cache 8kB 2-way, linesize 16 bytes.                                                
PID hash table entries: 64 (order 6: 512 bytes)                                               
Using 128.000 MHz high precision timer.                                       
Dentry cache hash table entries: 4096 (order: 2, 16384 bytes)                                                             
Inode-cache hash table entries: 2048 (order: 1, 8192 bytes)                                                           
Memory: 14112k/16000k available (1300k kernel code, 1868k reserved, 199k data, 7                                                                                
2k init, 0k highmem)                    
Calibrating delay loop... 253.44 BogoM                                    
Mount-cache hash table entries: 512 (order: 0, 4096 bytes)                                                          
Checking for 'wait' instruction...  unavailable.                                                
NET: Registered protocol family 16                                  
Can't analyze prologue code at 80153bbc                                       
Software Watchdog Timer: 0.07 initialized. soft_noboot=0 soft_margin=1 sec (nowa                                                                                
yout= 0)        
PPP generic driver version 2.4.2                                
NET: Registered protocol family 24                                  
Using noop io scheduler                       
bcm963xx_mtd driver v1.0                        
brcmboard: brcm_board_init entry                                
bcm963xx_serial driver v2.0                           
NET: Registered protocol family 2                                 
IP: routing cache hash table of 51                                
TCP: Hash tables configured (established 512 bind 1024)                                                       
NET: Registered protocol family 1                                 
NET: Registered protocol family 17                                  
Ebtables v2.0 registered                        
NET: Registered protocol family 8                                 
NET: Registered protocol family 20                                  
802.1Q VLAN Support v1.8 Ben Greear <greearb@candelatech.com>                                                             
All bugs added by David S. Miller <davem@redhat.com>                                                    
VFS: Mounted root (squashfs filesystem) readonly.                                                 
Freeing unused kernel memory: 72k freed                                       
init started:  BusyBox v1.00 (2006.04.05-12:12+0000) multi-call binary                                                                      
Algorithmics/MIPS FPU E                     

BusyBox v1.00 (2006.04.05-12:12+0000) Built-in shell (msh)                                                          
Enter 'help' for a list of built-in commands.                                             

Loading drivers and kernel modules...                                     

atmapi: module license 'Proprietary' taints kernel.                                                   
blaadd: blaa_detect entry                         
adsl: adsl_init entry                     
Broadcom BCMPROCFS v1.0 initialized                                   
Broadcom BCM6348B0 Ethernet Network Device v0.3 Apr  5 2006 20:08:56                                                                    
Config Internal PHY Through MDIO                                
BCM63xx_ENET: Auto-negotiation timed-out                                        
BCM63xx_ENET: 10 MB Half-Duplex (assumed)                                         
eth0: MAC Address: 00:16:38:FB:DD:2E                                    
Broadcom BCM6348B0 Ethernet Network Device v0.3 Apr  5 2006 20:08:56                                                                    
Config External PHY Through MDIO                                
Correc Ext PHY address: 19                          
BCM63xx_ENET: Auto-negotiation timed-out                                        
BCM63xx_ENET: 10 MB Half-Duplex (assumed)                                         
eth1: MAC Address: 00:16:38:FB:DD:2F                                    
Broadcom BCM6348B0 USB Network Device v0.4 Apr  5 2006 20:08:58                                                               
usb0: MAC Address: 00 16 38 FB DD 30                                    
usb0: Host MAC Address: 00 16 38 FB DD 31                                         
PCI: Setting latency timer of device 0000:00:01.0 to 64                                                       
PCI: Enabling device 0000:00:01.0 (0004 -> 0006)                                                
wl: srom not detected, using main memory mapped srom info (wombo board)                                                                       
wl0: wlc_attach: using main broad MAC address base in NVRAM (wombo board)                                                                         
wl0 MAC Address: 00:16:38:FB:DD:39                                  
wl0: Broadcom BCM4318 802.11 Wireless Controller 3.91.23.0                                                          
Endpoint: endpoint_init entry                             
BOS: Enter bosInit                  
BOS: Enter bosAppInit                     
BOS: Exit bosAppInit                    
BOS: Exit bosInit                 
Endpoint: endpoint_init COMPLETED                                 
AdslCoreHwReset: AdslOemDataAddr = 0xA0FFB2D4                                             

==>   Bcm963xx Software Version: AH4021.24.2.01.300L01.V04.mgcp.dspApp3341_fxo.L                                                                                
E9500A2pB019b10.d16m   <==                          

iptables v1.2.11: can't initialize iptables table `filter': iptables who? (do yo                                                                                
u need to insmod?)                  
Perhaps iptables or your kernel needs to be upgraded.                                                     
device usb0 entered promiscuous mode                                    
br0: port 1(usb0) entering learning state                                         
br0: topology change detected, propagating                                          
br0: port 1(usb0) entering forwarding state                                           
device eth0 entered promiscuous mode                                    
br0: port 2(eth0) entering learning state                                         
br0: topology change detected, propagating                                          
br0: port 2(eth0) entering forwarding state                                           
device eth1 entered promiscuous mode                                    
br0: port 3(eth1) entering learning state                                         
br0: topology change detected, propagating                                          
br0: port 3(eth1) entering forwarding state                                           
Unique ID: 6A374C427632617671586B45456C796867583358                                                   
Key Output: 6B 81 EE 16 94 2A 0B 1F AA 9F 1C 8A D9 B4 6F 2D 64 AF 5E 51                                                                       
Setting country code "FR"                         
device wl0 entered promiscuous mode                                   
br0: port 4(wl0) entering learning state                                        
br0: topology change detected, propagating                                          
br0: port 4(wl0) entering forwarding state                                          
br0: port 4(wl0) entering disabled stat                                     
br0: port 4(wl0) entering learning state                                        
br0: topology change detected, propagating                                          
br0: port 4(wl0) entering forwarding state                                          
device usb0 left promiscuous mode                                 
br0: port 1(usb0) entering disabled state                                         
device usb0 entered promiscuous mode                                    
br0: port 1(usb0) entering learning state                                         
br0: topology change detected, propagating                                          
br0: port 1(usb0) entering forwarding state                                           
device eth1 left promiscuous mode                                 
br0: port 3(eth1) entering disabled state                                         
device eth1 entered promiscuous mode                                    
br0: port 3(eth1) entering learning                                    
br0: topology change detected, propagating                                          
br0: port 3(eth1) entering forwarding state                                           
device wl0 left promiscuous mode                                
br0: port 4(wl0) entering disabled state                                        
device wl0 entered promiscuous mode                                   
br0: port 4(wl0) entering learning state                                        
br0: topology change detected, propagating                                          
br0: port 4(wl0) entering forwarding state                                          
device eth0 left promiscuous mode                                 
br0: port 2(eth0) entering disabled state                                         
device eth0 entered promiscuous mode                                    
br0: port 2(eth0) entering learning state                                         
br0: topology change detected, propagat                                      
br0: port 2(eth0) entering forwarding state                                           
sntp: host not found                    
Starting the MGCP application with the following parameters:                                                            

Call Agent IP address/FQDN: mgcr.libertysurf.net                                                
Gateway name: 00000000000000000000.mgcp                                       
Interface name: ppp_8_35_1                          
Preferred codec: auto                     
kernel::endpoint_open                     
kernel::endpoint_open COMPLETED                               
BOS: Enter bosInit                  
BOS: Enter bosAppInit                     
BOS: Exit bosAppInit                    
BOS: Exit bosInit                 
00:00:35 Calling callClient                           
try to probe the DNS server                           
app: /bin/dnsprobe &                    
00:00:35 ERROR resolving address mgcr.liberty                                           

=====================================================                                                     
MGCP Call Control, by Tommy Huang                                 
=====================================================                                                     

00:00:35 GWCONFIG Data:                       
00:00:35        CA_#1 Name  - ca@mgcr.libertysurf.net                                                     
00:00:35        CA_#2 Name  - ca@mgcr.libertysurf.net                                                     
00:00:35        CA_#3 Name  - ca@mgcr.libertysurf.net                                                     
00:00:35        GW Name     - 00000000000000000000.mgcp                                                       
00:00:35        Interface name  - ppp_8_35_1                                            
00:00:35        Preferred Codec  - auto                                       
00:00:35        Country  - FRA                              
00:00:35                       
00:00:35        CA Port  - 2427                               
00:00:35        MGC Port  - 2427                                
00:00:35        TX Gain  - 0                            
00:00:35        RX Gain  - 0                            
00:00:35        PSTN Access Code  - ##                                      
00:00:35        Heartbeat Timer  - 0                                    
00:00:35        Emergency List  - 112|115|119|15|17|18                                                      
00:00:35        FXS Reception port(3 means both)  - 3                                                     
Created queue HDSP                  
00:00:35 CALLCLIENT: Initializing endpoints                                           
app: echo 0 > /var/telephone0_status                                    
dnsprobe: Can not open /etc/resolv.conf                                       
app: echo 0 > /var/telephone1_status                                    
app: echo 0 > /var/mgcpstats                            
00:00:35 CALLCLIENT: Initializing endpoints                                           
00:00:35 Endpoint will be initialized for country FRA (country code = 5)                                                                        

00:00:35 Endpoint will be initialized for TX Gain: 0 dB, RX Gain: 0 dB                                                                      

00:00:35 Endpoint Event task started with pid 431...                                                    

BOS: Created task eptEvent                          
00:00:35 Endpoint Packet task started with pid 432 ...                                                      

BOS: Created task eptPacket                           
BOS: Enter bosStartApp                      

BOS: bosAppRootTask() - Is it morning already? Spawning app task (epoch #0)...                                                                              

BOS: Enter TaskCreate aoAP                          
BOS: TaskCreate - spawn new task a                                
bcmOsTaskCreate:                
 TASK NAME      = aoAP                      
 TASK_PRIORITY  = 1                   
BOS: Exit TaskCreate                    
BOS: AppResetDetectionEnable() - Enabled reset detection.                                                         
bcmOsTaskCreate:                
 TASK NAME      = aoRT                      
 TASK_PRIORITY  = 1                   
BOS: Exit bosStartApp                     
Reseting the 3341                 
voipResetGpio = 6                 
PASS: mmr         
PASS: chipCtl             
PASS: mspi          
PASS: scratchSram                 
PASS: apmregs             
PASS: apm0          
PASS: apm1          
PASS: hvg         
PASS: slic          
PASS: vpm         
PASS: mbox          
3341 diagnostics passed!                        
Reseting the 3341                 
voipResetGpio = 6                 
Initializing 3341 drivers                         
-------------- TDM DMA setup strt --------------                                                
SAMPLESIZE = 8              
DESCRIPTORP = 0xb7fe6300 INGRESSP = 0xb7fe6310 EGRESSP = 0xb7fe6330                                                                   
Initializing Memory: 8 (16-bit locations)                                         
Priming TX FIFO....                   
Completed TDM3341 init!!!!                          
MSPI driver init SUCCESSFUL                           
MSPI driver registers update SUCCESSFUL                                       
BOARDHAL Enabling relays                        
Loading 3341 Zsp with Hausware app.                                   
Loading 3341 overlay to 0xb7fc0000.